SEQ7016 -- 16 Channel Video & Audio DVR

Features:

User-friendly menu and easy to operate

Support up to 1360X768 VGA resolution

Support digital zoom when preview,playback and PTZ mode

Different channels can be set different recording expired time

Support normal and event video encoding parameters

Support redundant recording

Support hard disk group management

Support Mobile View function

Support multi-playback function

Support disk-saver function

Support CMS function

Specs:

Image Housing Height: 1U

Operation System: Linux

Video Input: 16 channels video input

Video Output: BNC video output, 1 VGA output

Audio Input: 16 channels audio input

Audio Output: 1 BNC audio output, Voice Talk/3.5mm Mic Interface

Playback: 4ch

Total Frames: PAL:400fps/NTSC:480fps

Compression Algorithm:: Video: H.264 / Audio: G.711 or G.722 or G.726

Record Resolution:: CIF: PAL (352*288), NTSC (352*240)

Preview Resolution: 4CIF(PAL:704*576,NTSC:704*480)

VGA: Up to 1360*768

Dual Stream: Yes

Image Quality: 6 levels optional

HDD: 2 SATA interfaces ( Each HDD can max support 2000GB)

Alarm Input: 16 alarm inputs

Alarm Output: 2 alarm outputs

Backup Interface: USB2.0 / High Speed SATA / Remote Backup

Digital Zoom: Yes

Mobile View: Yes( Supporting Windows Mobile, Symbian and iPhone System)

Network Interface: RJ45 10M/100M Ethernet Interface

I/O Interface: RX485/RS485, RS485 for PTZ

USB for Mouse

Other Functions

Watchdog / Dual Stream / PPPoE / DHCP / DDNS

Power Supply: 220±30% V, 50±3% Hz or 110±20% V, 60±3% Hz

Power Consumption: 11W (without hard disk)

Work Temperature: - 10℃～ +55℃

Working Humidity: 10% ～ 90%

Dimension: 405mm*310mm*55mm

Gross weight: 5.5KG ( without hard disk)